MAINTENANCE CHECKLIST JAGUAR F-TYPE 2024 MY 5.0 L 

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Service interval TIME (years) | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 |
| Interval: Miles x 1000 | 16 | 32 | 48 | 64 | 80 | 96 | 112 | 128 | 144 | 160 |
| Interval: Km x 1000 | 26 | 52 | 78 | 104 | 130 | 156 | 182 | 208 | 234 | 260 |
| Check for and complete all open Recalls and Service Actions | O | O | O | O | O | O | O | O | O | O |
| Check wiper blades condition; operation of washer/wiper system | O | O | O | O | O | O | O | O | O | O |
| Check and top up underhood fluid levels | O | O | O | O | O | O | O | O | O | O |
| Check and top up windshield washer resevoir | O | O | O | O | O | O | O | O | O | O |
| Check for underhood / undervehicle fluid leaks | O | O | O | O | O | O | O | O | O | O |
| Check all tyre pressures, condition, tread depth, signs of uneven wear and suitability | O | O | O | O | O | O | O | O | O | O |
| Check brake pad wear, check disc condition on pad change | O | O | O | O | O | O | O | O | O | O |
| Check tyre repair system fluid expiry date, replace if date before next service |  |  | O |  |  | O |  |  | O |  |
| Replace engine oil and filter | O | O | O | O | O | O | O | O | O | O |
| Replace engine air cleaner element |  |  |  | O |  |  |  | O |  |  |
| Replace interior air filter element |  | O |  | O |  | O |  | O |  | O |
| Replace brake fluid |  | O |  | O |  | O |  | O |  | O |
| Replace spark plugs |  |  |  |  |  | O |  |  |  |  |
| Replace engine coolant |  |  |  |  |  |  |  |  |  | O |
| Replace front accessory drive belt |  |  |  |  |  |  |  |  | O |  |
| Replace supercharger belt |  |  |  |  |  |  |  |  | O |  |
| Replace transmission oil and filter |  |  |  |  |  |  |  |  | O |  |
| Replace transfer case oil |  |  | O |  |  | O |  |  | O |  |
| Replace front differential oil |  |  |  |  |  |  |  |  | O |  |
| Replace rear locking differential oil |  |  |  | O |  |  |  | O |  |  |
| Perform comprehensive road test; check operation of all vehicle features: Park brake, seatbelts, steering column , seats, mirrors, starter motor, instruments, lamps, horn, warning indicators, transmission control interlock, steering self centre, steering wander, transmission shifts, brakes, cruise control, climate control, undue noises. | O | O | O | O | O | O | O | O | O | O |
| Reset service indicator and oil level indicators | O | O | O | O | O | O | O | O | O | O |
| Fault lamp(s) illuminated? If 'yes', use a Jaguar approved diagnostic tool for diagnosis/repair | O | O | O | O | O | O | O | O | O | O |
| Report any unusual features of vehicle condition and additional work required | O | O | O | O | O | O | O | O | O | O |
| Endorse service record | O | O | O | O | O | O | O | O | O | O |